---
type: Known
product: PAN-OS
version: 11.0.4
---

## WF500-5632

The number of registered WildFire appliances
reported in Panorama (PanoramaManaged WildFire AppliancesFirewalls ConnectedView) does not accurately reflect the
current status of connected WildFire appliances.

## PAN-260851

From the NGFW or Panorama CLI, you can override the existing
application tag even if Disable Override is enabled for the
application (ObjectsApplications) tag.

## PAN-234015

The X-Forwarded-For (XFF) value is not displayed in traffic logs.

## PAN-252744

After upgrading PA-3200 Series, PA-5200 Series, or PA-7000 Series
firewalls that are equipped with OCTEON 7x00 dataplane chips to
PAN-OS 11.0.4 or 11.0.4-h1, the firewall might see continuous
crashes, reboot repeatedly, and/or go into a non-functional
state.

Workaround: If you have already upgraded to one of those
releases, downgrade to an earlier release or upgrade to PAN-OS
11.0.4-h2.

## PAN-241041

On the Panorama management server exporting template or template
stack variables (PanoramaTemplates) in CSV format results in an empty CSV file.

## PAN-234929

The tabs in the ACC, such as
Network Activity, Threat
Activity, and Blocked
Activity, may not display any data when you apply a
Time filter for the Last 15 minutes, Last Hour, Last 6 Hours, or
Last 12 Hours. With the Last 24 Hours filter, the data displayed may
not be accurate. Additionally, reports run against summary logs may
not display accurate results.

## PAN-225886

If you enable explicit proxy mode for the web proxy, intermittent
errors and unexpected TCP reconnections may occur.

## PAN-233677

```caveat
PA-3410, PA-3420, PA-3430, PA-3440, PA-5410, PA-5420, PA-5430, and PA-5440 firewalls
```

By enabling Lockless QoS feature, a
slight degradation in App-ID and Threat performance is expected.

## PAN-222586

On PA-5410, PA-5420, PA-5430, and PA-5440 firewalls, the Filter
dropdown menus, Forward Methods, and Built-In Actions for
Correlation Log settings (DeviceLog Settings) are not displayed and cannot be configured.

## PAN-222253

On the Panorama management server, policy rulebase reordering when
you View Rulebase by Groups (Policy<policy-rulebase>) does not persist if you reorder the policy rulebase
by dragging and dropping individual policy rules and then moving the
entire tag group.

## PAN-221033

The firewall is responding to an ARP request for an IP address in the
firewall's NAT address pool when that IP address isn't in the same
subnet as the IP address of the ingress interface.

## PAN-220176

```caveat
PAN-OS 11.0.1-h2 hotfix
```

System process crashes might occur
with VoIP traffic when NAT is enabled with Persistent Dynamic IP and
Port settings.

## PAN-218521

The ElasticSearch process on the M-600 appliance in Log Collector
mode may enter a continuous reboot cycle. This results in the M-600
appliance becoming unresponsive, consuming logging disk space, and
preventing new log ingestion.

## PAN-216314

Upon upgrade or downgrade to or from PAN-OS 10.1.9 or 10.1.9-h1,
offloaded application traffic sessions may disconnect after a period
of time even if a session is active. The disconnect occurs after the
application's default session timeout value is exceeded. This
behavior affects only PAN-OS 10.1.9 and 10.1.9-h1. If you are on
PAN-OS 10.1.9 and 10.1.9-h1, please use the following workaround. If
you have already upgraded or downgraded to another PAN-OS version,
use the following workaround in that version.

Workaround: Run the CLI command debug dataplane
internal pdt fe100 csr wr_sem_ctrl_ctr_scan_dis value
0 to set the value to zero (0).

## PAN-216214

For Panorama-managed firewalls in an Active/Active High Availability
(HA) configuration where you configure the firewall HA settings (DeviceHigh Availability) in a template or template stack (PanoramaTemplates), performing a local commit on one of the HA
firewalls triggers an HA config sync on the peer firewall. This
causes the HA peer configuration to go Out of
Sync.

## PAN-213746

On the Panorama management server, the Hostkey
displayed as undefined undefined if you
override an SSH Service Profile (DeviceCertificate ManagementSSH Service Profile) Hostkey configured in a Template from the Template
Stack.

## PAN-213119

PA-5410 and PA-5420 firewalls display the following error when you
view the Block IP list (MonitorBlock IP):

show -> dis-block-table is
unexpected

## PAN-212978

The Palo Alto Networks firewall stops responding when executing an
SD-WAN debug operational CLI command.

## PAN-212889

On the Panorama management server, different threat names are used
when querying the same threat in the Threat Monitor (MonitorApp ScopeThreat Monitor) and ACC. This results in the
ACC displaying no data to display when
you are redirected to the ACC after clicking a threat name in the
Threat Monitor and filtering the same threat name in the Global
Filters.

## PAN-211531

On the Panorama management server, admins can still
perform a selective push to managed firewalls when Push All
Changes and Push for Other Admins
are disabled in the admin role profile (PanoramaAdmin Roles).

## PAN-207770

Data filtering logs (MonitorLogsData Filtering)
incorrectly display the traffic Direction as server-to-client instead
of client-to-server for upload traffic
that matches Enterprise data loss prevention (DLP) data patterns (ObjectsDLPData
Filtering Patterns) in an Enterprise DLP data
filtering profile (ObjectsDLPData Filtering Profiles).

## PAN-207733

When a DHCPv6 client is configured on HA
Active/Passive firewalls, if the DHCPv6 server goes down, after
the lease time expires, the DHCPv6 client should enter SOLICIT state
on both the Active and Passive firewalls. Instead, the client is
stuck in BOUND state with an IPv6 address having lease time 0 on
the Passive firewall.

## PAN-207616

On the Panorama management server, after
selecting managed firewalls and creating a new Tag (PanoramaManaged DevicesSummary) the managed firewalls are
automatically unselected and any new tag created is applied to the
managed firewalls for which you initially created the new tag.

Workaround: Select
and then unselect the managed firewalls for which you created a
new tag.

## PAN-207611

When a DHCPv6 client is configured on HA
Active/Passive firewalls, the Passive firewall sometimes crashes.

## PAN-207442

For M-700 appliances in an active/passive high availability (PanoramaHigh Availability) configuration, the
active-primary HA peer
configuration sync to the
secondary-passive HA peer may fail.
When the config sync fails, the job Results is
Successful
(Tasks), however the sync status on the
Dashboard displays as Out
of Sync for both HA peers.

Workaround: Perform a local commit on the
active-primary HA peer and then
synchronize the HA configuration.

1. Log in to the Panorama
  web interface of the
  active-primary HA peer.
2. Select Commit and Commit to
  Panorama.
3. In the active-primary HA peer
  Dashboard, click Sync
  to Peer in the High Availability widget.

## PAN-207040

If you disable Advanced Routing, remove
logical routers, and downgrade from PAN-OS 11.0.0 to a PAN-OS 10.2.x
or 10.1.x release, subsequent commits fail and SD-WAN devices on
Panorama have no Virtual Router name.

## PAN-206913

When a DHCPv6 client is configured on HA
Active/Passive firewalls, releasing the IPv6 address from the client
(using Release in the UI or using the request dhcp client ipv6 release all CLI
command) releases the IPv6 address from the Active firewall, but
not the Passive firewall.

## PAN-206909

The Dedicated Log Collector is unable to
reconnect to the Panorama management server if the configd process
crashes. This results in the Dedicated Log Collector losing connectivity
to Panorama despite the managed collector connection Status (PanoramaManaged Collector)
displaying connected and the managed colletor Health status displaying
as healthy.

This results in the local Panorama config and
system logs not being forwarded to the Dedicated Log Collector.
Firewall log forwarding to the disconnected Dedicated Log Collector
is not impacted.

Workaround: Restart the mgmtsrvr process
on the Dedicated Log Collector.

1. Log in to the Dedicated Log Collector
  CLI.
2. Confirm the Dedicated Log Collector is disconnected from
  Panorama.
  admin> show panorama-status
  Verify
  the Connected status is no.
3. Restart the mgmtsrvr process.
  admin> debug software restart process management-server

## PAN-206416

On the Panorama management server, no data
filtering log (MonitorLogsData Filtering) is generated
when the managed firewall loses connectivity to the following cloud services,
and as a result fails to forward matched traffic for inspection.

- DLP cloud service
- Advanced Threat Protection inline cloud analysis service
- Advanced URL Filtering cloud service

## PAN-206315

```caveat
PA-1420 firewall only
```

In an active/passive high
availability (HA) configuration, the show session info CLI
command shows that the passive firewall has packet rate and throughput
values. The packet rate and throughput of the passive firewall should
be zero since it is not processing traffic.

## PAN-205009

```caveat
PA-1420 firewall only
```

In an active/passive high
availability (HA) configuration, the show interface all, show-high availability interface ha2,
and show high-availability all CLI
commands display the HSCI port state as unknown on both the active
and passive firewalls.

## PAN-204689

Upon upgrade to PAN-OS 11.0.1, the following GlobalProtect settings
do not work:

- Allow user to disconnect GlobalProtect
  AppAllow with Passcode
- Allow user to Disable GlobalProtect
  AppAllow with Passcode
- Allow User to Uninstall GlobalProtect
  AppAllow with Password

## PAN-201910

PAN-OS security profiles might consume a
large amount of memory depending on the profile configuration and
quantity. In some cases, this might reduce the number of supported security
profiles below the stated maximum for a given platform.

## PAN-197588

The PAN-OS ACC (Application Command Center)
does not display a widget detailing statistics and data associated
with vulnerability exploits that have been detected using inline
cloud analysis.

## PAN-197419

```caveat
PA-1400 Series firewalls only
```

In NetworkInterfaceEthernet, the power over Ethernet
(PoE) ports do not display a Tag value.

## PAN-197097

Large Scale VPN (LSVPN) does not support
IPv6 addresses on the satellite firewall.

## PAN-196758

On the Panorama management server, pushing
a configuration change to firewalls leveraging SD-WAN erroneously
show the auto-provisioned BGP configurations for SD-WAN as being
edited or deleted despite no edits or deletions being made when
you Preview Changes (CommitPush to DevicesEdit Selections or CommitCommit and PushEdit Selections).

## PAN-196146

The VM-Series firewall on Azure does not
boot up with a hostname (specified in an init-cgf.txt or user data)
when bootstrapped.

## PAN-195968

```caveat
PA-1400 Series firewalls only
```

When using the CLI to configure power over Ethernet (PoE) on a non-PoE
port, the CLI prints an error depending on whether an interface
type was selected on the non-PoE port or not. If an interface type, such
as tap, Layer 2, or virtual wire, was selected before PoE was configured,
the error message will not include the interface name (eg. ethernet1/4).
If an interface type was not selected before PoE was configured,
the error message will include the interface name.

## PAN-195342

On the Panorama management server, Context
Switch fails when you try to Context Switch from a managed firewall running
PAN-OS 10.1.7 or earlier release back to Panorama and the following
error is displayed:

Could not find start token '@start@'

## PAN-194978

```caveat
PA-1400 Series firewalls only
```

In NetworkInterfaceEthernet, hovering the mouse over
a power over Ethernet (PoE) Link State icon
does not display link speed and link duplex details.

## PAN-194424

```caveat
PA-5450 firewall only
```

Upgrading
to PAN-OS 10.2.2 while having a log interface configured can cause
both the log interface and the management interface to remain connected
to the log collector.

Workaround: Restart the log receiver service
by running the following CLI command:

debug software restart process log-receiver

## PAN-187685

On the Panorama management server, the Template Status
displays no synchronization status (PanoramaManaged DevicesSummary)
after a bootstrapped firewall is successfully added to Panorama.

Workaround: After
the bootstrapped firewall is successfully added to Panorama, log in to the Panorama web interface and
select CommitPush
to Devices.

## PAN-187407

The configured Advanced Threat Prevention
inline cloud analysis action for a given model might not be honored
under the following condition: If the firewall is set to Hold
client request for category lookup and the action set
to Reset-Both and the URL cache has been
cleared, the first request for inline cloud analysis will be bypassed.

## PAN-186283

Templates appear out-of-sync on Panorama
after successfully deploying the CFT stack using the Panorama plugin for
AWS.

Workaround: Use CommitPush to Devices to synchronize
the templates.

## PAN-184708

```caveat
Panorama managed firewalls
```

Scheduled report emails (MonitorPDF ReportsEmail Scheduler) are not emailed if:

- A scheduled report email contains
  a Report Group (MonitorPDF
  ReportsReport Group)
  which includes a SaaS Application Usage report.
- A scheduled report contains only a SaaS Application Usage Report.

Workaround: To
receive a scheduled report email for all other PDF report types:

1. Select MonitorPDF ReportsReport Groups and
  remove all SaaS Application Usage reports from all Report Groups.
2. Select MonitorPDF
  ReportsEmail Scheduler and
  edit the scheduled report email that contains only a SaaS Application Usage
  report. For the Recurrence, select Disable and
  click OK.
  Repeat this step for all scheduled
  report emails that contain only a SaaS Application Usage report.
3. Commit.
  ()
  Select CommitCommit
  and Push

## PAN-184406

Using the CLI to add a RAID disk pair to
an M-700 appliance causes the dmdb process to crash.

Workaround: Contact
customer support to stop the dmdb process before adding a RAID disk
pair to a M-700 appliance.

## PAN-183404

Static IP addresses are not recognized when
"and" operators are used with IP CIDR range.

## PAN-181933

If you use multiple log forwarding cards
(LFCs) on the PA-7000 series, all of the cards may not receive all
of the updates and the mappings for the clients may become out of sync,
which causes the firewall to not correctly populate the Source User
column in the session logs.

## PAN-171938

No results are displayed when you Show Application
Filter for a Security policy rule (PoliciesSecurityApplicationValueShow Application Filter).

## PAN-164885

On the Panorama management server, pushes to managed firewalls (CommitPush to Devices or Commit and Push) may fail
when an EDL (ObjectsExternal Dynamic Lists) is configured to Check for
updates every 5 minutes due to the commit and EDL
fetch processes overlapping. This is more likely to occur when
multiple EDLs are configured to check for updates every 5
minutes.
